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Cardboard Specification
This cardboard specification relates to all cardboard received at E Team Ltd. This covers:
· Loose
· Small bales 
· Mill-sized bales
· Skip/Compactor loads
Customers should produce material which meets the following specifications within the tolerances set out below. 
Mill-sized bales should contain uniform material to meet the material specification. 
	3% Tolerance

	Newspapers 
Magazines and pamphlets 
Grey and brown carton board 
Kraft paper 
White office paper 
Printers waste 
Envelopes 
Catalogues 
Books 
Telephone directories 
Soft cores

	[bookmark: _GoBack]Unwanted Material
	Prohibitive

	There is no tolerance for any of the following and loads may be subject to a handling or disposal fee if present:

Metals
Cans
Plastic bottles and cups
Plastic film/polystyrene
Plastic rigids
Any other plastic
Pallet strapping
Wall paper
Wax/Label Paper
Carbon paper
Tetrapak
Self-adhesive paper
Hand Towels
Tissue paper

	There is no tolerance for any of the following and loads may be rejected if present:

Poly-coated Cardboard (plastic coating printed on cardboard)
Food Waste 
Egg cartons/boxes
Garden Waste
Gloves
Medical Hygiene Waste
Hazardous Materials (e.g. paint, chemicals, oil, asbestos)
Nappies
Concrete, soil, stone and brick
Glass
Bitument
Wood & pallets
Electrical equipment/cable
Textiles
Rubber
Batteries



Cleanliness: 	Material must be free of dirt, grit, fire damage and should not be mouldy
Moisture: 	Cardboard must be kept dry and could be subject to moisture claims if wet
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